XP Universal Driver U M

## Edge Acceleration Tool (EAT)

Edge Acceleration tool can be used to configure cursor acceleration towards the edge of the touchscreen. Edge Acceleration is a special feature provided to allow touches towards the edges.

EAT (i.e. EloAccel.exe) can be launched from Program Files> EloTouchsystems folder.

Presents a full screen image with the edge acceleration rectangle bounds and a Cursor Acceleration Configuration dialog, displaying the configuration parameters for Edge Acceleration.

Configurable parameters are:

- Cursor Acceleration scale. This scale can be set from a value of 0-10 where, 1 corresponds to no acceleration.
- Edge acceleration rectangle bounds dimensions.
- Edge acceleration rectangle bounds position
- Enable Edge acceleration

Cursor is accelerated beyond the rectangle bounds.

These parameters can be configured using mouse, to resize or move the bounds rectangle or, by entering the values directly in the dialog box. Changes to the settings in the Cursor Acceleration dialog take effect when the "Apply" button is clicked.

This applies to all touchmonitors unless run with appropriate command line options. To view the options available, run EloAccel using EloAccel /h.