
[Version]
Signature="$Windows NT$"
Provider=%ps2aux%
ClassGUID={4D36E96F-E325-11CE-BFC1-08002BE10318}
Class=Mouse
CatalogFile=ps2aux.cat
DriverVer=04/15/2002, 6.01

[ClassInstall32]
AddReg=mouse_class_addreg

[mouse_class_addreg]
HKR,,Icon,,"-2" 
HKR,,Installer32,,"SysSetup.Dll,MouseClassInstaller" 
HKR,,NoInstallClass,,"1" 

[DestinationDirs]
DefaultDestDir   = 12

;
; Driver information
;

[Manufacturer]
%ps2aux%   = ps2aux.Mfg

[ps2aux.Mfg]
%ps2aux% TouchScreen = ps2aux, *PNP0FAKE
%ps2aux% TouchScreen = ps2aux, ACPI\PNP0F13

;
; General installation section
;

[ps2aux]
; perform port related actions from msmouse.inf
Include=msmouse.inf
Needs=PS2_Inst

; Copy the driver over
CopyFiles=ps2aux.CopyFiles


;
; File sections
;

[ps2aux.CopyFiles]
ps2aux.sys


;
; Service Installation
;

[ps2aux.Services]
AddService = ps2aux,  , ps2aux_Service_Inst
; Install the port driver and mouclass from msmouse.inf
Include=msmouse.inf
Needs=PS2_Inst.Services

[ps2aux_Service_Inst]
DisplayName    = %ps2aux.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 0                  ; SERVICE_ERROR_IGNORE
LoadOrderGroup = Pointer Port
ServiceBinary  = %12%\ps2aux.sys

[ps2aux.HW]
; Add the device upper filter
AddReg = ps2aux.HW.AddReg

; run the directives need by the port driver
Include=msmouse.inf
Needs=PS2_Inst.HW

[ps2aux.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"ps2aux"


;
; Source file information
;

; use [SourceDisksNames.x86] for x86 only installs
; use [SourceDisksNames.alpha] for alpha only installs

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
ps2aux.sys = 1,,


[Strings]

;
; Non-Localizable Strings
;

REG_SZ         = 0x00000000
REG_MULTI_SZ   = 0x00010000
REG_EXPAND_SZ  = 0x00020000
REG_BINARY     = 0x00000001
REG_DWORD      = 0x00010001
SERVICEROOT    = System\CurrentControlSet\Services

;
; Localizable Strings
;

DiskId1 = "PS2 Installation Disk #1 (TouchScreen)"
ps2aux = "PS2"
%ps2aux.SvcDesc%="PS2 Touch Screen"

